## Here is an easy way to tell if a 280T/280W meter is **Modbus** output or **RS485** for BACnet.

Connect the module to computer through USB adapter with 12VDC power and read with MBSheet. If it can be read, it is RS485; if it cannot read, it is Modbus.